**CHASSIS:**

|  |
| --- |
| 2018 Model Year or NewerLess than 18,000 miles276" Wheel Base |
| Front And Rear Tow Hooks |
| Heavy Duty Front Bumper |
| Front Electric Crossing Gate |
| 10,000 Lbs Front Axle |
| 10,000 Lbs Front Springs |
| Antilock Hydraulic Brakes W/ Traction Control |
| Disc Brakes Front And Rear |
| 12x3 Bosch Parking Park With Interlock |
| Power Steering |
| Tilt Steering Column |
| Single Exhaust With LH Exit Tailpipe |
| Heat Shield For Exhaust |
| Dual Electric Horns |
| Daytime Running Lights |
| 200amp Bosch Alternator |
| (3) Batteries - 1950 CCA Total |
| Delco Remy 12 Volt Starter |
| Aero Halogen Headlights |
| Low Coolant Alarm  |
| Manual Reset Circuit Breakers |
| Wig Wag Headlights |
| Tilt Hood And Fenders, Easy Tilt |
| **Cummins ISB EPA 16 Electronic Controlled** |
| Turbo Charger / After Cooled Diesel Engine |
| **240 HP 560 Ft/Lbs Torque** |
| 750 Watt Block Heater |
| Warner Electric Fan Drive |
| Engine Oil Cooler |
| Engine Noise Abatement Package |
| Heavy Duty Dry Air Cleaner |
| Keyed Alike Ignition Switch |
| Electronic Fast Idle |
| Cruise Control |
| Eaton Procision Transmission  |
| Push Button Shift Controls |
| Synthetic Transmission Fluid |
| 19,800 Lbs Rear Axle |
| 19,800 Lbs Rear Spring Suspension |
| 5.29 Gear Ratio |
| Synthetic Fluid In Front Oil Hubs And Rear Axle |
| Front And Rear Shock Absorbers |
| 100gal BFR Fuel Tank |
| 12 Gal DEF Tank |
| Fuel Filter |
| Transmission Temp Gauge |
| Ammeter / Def Level Gauge |
| Speedometer / Odometer / Tachometer |
| Hourmeter / Oil Pressure / Water Temp |
| Fuel Level Gauge Display |
| On Board IP Diagnostic Display |
| 22.5" X 8.25" HUB POLITED WHEELS |
| Oil Lubed Front Wheel Seals |
| 11R22.5 Tires – Steer Tread Front, Mud/Snow Tread Rear |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **Body** |
|  |
|  |
| 33'5" Body Length |
| FMVSS Body Construction |
| 78" Interior Headroom |
| Full Length Perforated Headliner |
| Headliner Fastened With Screws |
| Lettering To Federal And Kansas Requirements |
| 16 Gauge Exterior Smooth Side Panels |
| 16 Gauge 20" Skirt Panels |
| 14 Gauge Roof Bows |
| 4 Exterior Rub Rails With Top Edge Sealed |
| Rear Emergency Door With Retainer |
| Lower Glass In Rear Emergency Door |
| Rear Painted Bumper 12" High |
| Electric Open Out Entrance Door With Vandal Lock – **NO EXCEPTIONS** |
| Exterior Assist Handle For Entrance Door |
| Dual Door Controls Mounted On Steering Wheel & LH Switch Panel – **NO EXCEPTIONS**

|  |
| --- |
| Post Trip Inspection Monitor W/ Alarm |
| Insulation In Roof And Side 1.50" |
| Full Body Undercoating |
| Reflective Tape Around All Emergency Exits |
| 90,000 Btu Driver Heater / Defroster |
| 3 Piece Flat Windshield With Tinted Bank |
| Koroseal Flooring With Pebble Step Treads |
| ABS Plastic Wheelhose Covers |
| 2 Auxiliary Defroster Fans |
| 50,000 BTU Stepwell Heater / Defroster |
| 84,500 BTU Rear Underseat Heater |
| Heater Booster Pump |
| 1/4" Heater Vaves Under Hood |
| Static Roof Vent |
| Constant Torque Clamps On Heater Hoses |
| Full Width Defroster |
| Entrance / Emergency Door Header Pads |
| DOT SB High Back Barriers |
| DOT SB High Back Seat Belt Ready Seats |
| Modesty Panel Under Rh Barrier |
| Entrance Door Handrail Rh Barrier |
| National 2000 Driver Seat With Cloth Insert |
| Adjustable Height Belt With Orange Webbing |
| 7" Clear Back Up Lights |
| 7" Amber Front Directional Lights |
| 7" Rear Amber Directional Lights |
| Halogen 7" Red And Amber 8 Way Warning Lights |
| Black Paint Around 8 Way Lights |
| 4" Red Rear Stop/Tail Light With License Plate Light |
| 7" Red Rear Stop/Tail Lights |
| Armored Side Directional Lights |
| Armored Clearance And Cluster Lights- Led |
| Rear Door Pilot Light And Buzzer |
| Stepwell Light Wired To Clearance Lights |
| Magnetic Body Cut Off Solenoid |
| Exterior Light Check System |
| Drivers Dome Light |
| Plastic Light Bars |
| Sequentail Operation Warning System |
| Electric Stop Arm - Octagon With Led Lights |
| 6x30 Interior Rearview Mirror |
| 6x30 Interior Sunvisor |
| Kansas Safety Equipment |
| Noise Suppression Switch |
| Low Profile Strobe Light |
| Non Locking Fuel Door Latch |
| Wet Arm Washer System - 6qt Bottle With Single Switch |
| Reflectors As Required |
|  |

 |
|  |

 |
|  |
| **Additional Features** |
|  |
| Rear Door Vandal Lock |
| 3m Diamond Grade School Bus Signs |
| 3m Diamond Grade Reflective Tape - Sides And Exits And Rear |
| Keyed Alike Entrance, Battery, Fuel, & Electrical Doors |
| Noise Reduction In Roof Bows |
| Stepwell Insulation |
| Roof Bow Reinforcement |
| Stainless Steel Fasteners On Exterior Body Lights |
| 5/8" Exterior Grade Plywood Flooring |
| (4) Emergency Push Out Windows |
| (2) Specialty Roof Hatches |
| 28% Tinted Laminated Passenger Windows |
| Grey Floor And Step Treads |
| Grey Prevail Fireblock Upholstry |
| Storm Glass In Driver Window |
| Storm Glass In Upper And Lower Entrance Door |
| Storm Glass 1st Window Aft Entrance Door |
| Padded Shoulder Rails |
| 2" White No Standee Line In Floor |
| Driver Heater Deflector |
| Crossing Gate Interrupt Switch |
| Back Up Alarm 112db |
| Manual Resetting Circuit Breakers |
| 12 Volt Power Source |
| AM/FM/CD/PA Radio With 4 Speakers |
| Exterior PA Speaker |
| Rosco Openview Heated Remote Rearview Mirrors |
| Rosco Heated Crossview Mirrors |
| Double Row Of Dome Lights |
| 3" Rear ICC Light |
| Rear Dome On Separate Switch |
| 16 Lamp Light Monitor |
| Pre Wire For Video And Two Way Radio |
| Battery Cut Off Switch Located In Battery Compartment |
| 8 Way Light Hoods |
| Front Bulkhead Storage Compartment |
| Rear Bulkhead Access Door |
| Rear Rubber Fenders |
| Front And Rear Mud Flaps |
|  |